{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["Hárok1","Hárok2","Hárok3"],"not_rendered":{"charts":0,"images":3,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Hárok1","index":0,"n_rows":40,"n_cols":9,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["Záložné zdroje k teplovodným krbom",{"$nulls":6},"veľkoobchod"]
[{"$nulls":8},"\"  €\""]
["Záložný zdroj                                                                 NZ UNI",null,null,"NZ500",null,"NZ UNI"]
["Sieť ",null,null,"200-240V 40-60Hz",null,"200-240V 40-60Hz"]
["Batéria",null,null,null,"12V, 30-150Ah /olovený akumulátor/"]
["Menič:",null,null,"12Vss./230Vst./50Hz"]
["Max.výkon meniča:",null,null,"500W",null,"200W"]
["Pripojenie čerpadla:",null,null,"300W",null,"150W"]
["Rozmery ",null,null,"155x160x210mm",null,"125x160x210mm"]
["Hmotnosť:",null,null,"8kg",null,"4kg"]
[]
["Cena bez DPH:",null,null,155.35,"€",138.78,"€"]
{"$rows_empty":14}
["Prístroj zálohuje sieť. Napätie 230V50Hz."]
["Ak je prítomné sieťové napätie prístroj dobíja pripojený akumulátor a udržuje ho v nabitom stave,"]
["čerpadlo je napájané zo siete."]
["Ak dôjde k výpadku el.siete,prístroj sa automaticky prepne na menič, ktorý z akumulátoru vyrába "]
["chýbajúce sieťové napätie."]
[]
[]
[]
[]
["Tuma invest spol. s r.o., Partizánska 300/32, Bánovce nad Bebravou 95701"]
["e-mail.:tumainvest@gmail.com",null,null,"www.krby-tuma.sk"]
["tel.:0905 394055, 0918 995337",null,null,"www.kominy-tuma.sk"]
["tel.:046 5431611",null,null,"www.edilkamin-slovakia.sk"]
["fax.:046 5461611",null,null,"www.hoyan.sk"]

{"sheet":"Hárok2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"Hárok3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}