{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["Hárok1","Hárok2","Hárok3"],"not_rendered":{"charts":0,"images":25,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Hárok1","index":0,"n_rows":302,"n_cols":7,"rows_kept":302,"cut":false,"hidden":false,"merged":[[184,0,184,4],[266,0,266,4],[266,5,266,10],[196,0,196,4],[196,5,196,10],[208,0,208,4],[208,5,208,10],[220,0,220,4],[220,5,220,10],[254,0,254,4],[254,5,254,10],[242,0,242,4],[242,5,242,10],[158,0,158,4],[158,5,158,10],[178,0,178,10],[180,4,180,10],[179,0,179,10],[17,5,17,10],[28,5,28,10],[125,0,125,4],[125,5,125,10],[109,0,109,4],[109,5,109,10],[76,0,76,4],[76,5,76,10],[87,0,87,4],[87,5,87,10],[98,0,98,4],[98,5,98,10],[39,5,39,10],[50,5,50,10],[39,0,39,4],[17,0,17,4],[0,0,0,10],[2,4,2,10],[3,4,3,10],[4,4,4,10],[6,5,6,10],[1,0,1,10],[5,0,5,10],[6,0,6,4],[278,0,278,4],[278,5,278,10],[290,0,290,4],[290,5,290,10],[28,0,28,4],[136,0,136,4],[136,5,136,10],[147,0,147,4],[147,5,147,10],[50,0,50,4],[184,5,184,10],[65,0,65,4],[65,5,65,10],[181,4,181,10],[182,4,182,10],[183,0,183,10]],"flags":["formulas_cached_only"]}
["Teplovzdušné pece na pelety ARTEL"]
["Veľkoobchodný cenník bez DPH"]
[{"$nulls":4},"tel.: 0905 394055 , 046 5431611 , fax.: 046 5431612"]
[{"$nulls":4},"e-mail.: tumainvest@gmail.com"]
[{"$nulls":4},"web.: www.krby-tuma.sk"]
["Výhradný distribútor ARTEL pre SR "]
["Artel LS 8 IDRA - Oceľ",{"$nulls":4},"cena : 1848,74 €"]
[{"$nulls":5},"Rozmery: (ŠxVxH) 605x1015x565 mm"]
[{"$nulls":5},"Hmotnosť : 100 kg"]
[{"$nulls":5},"Výkon : 10,1 kW"]
[{"$nulls":5},"Menovitý tepelný výkon : 3,88 - 8,54 kW"]
[{"$nulls":5},"Prívod vzduchu priemer rúry : 50 mm"]
[{"$nulls":5},"Priemer potrubia dymu zásuvky : 80 mm"]
[{"$nulls":5},"Vyhrievatelná plocha : 120 m2"]
[{"$nulls":5},"Doba samostatnej prevádzky : 6,5 - 14 hodín"]
[{"$nulls":5},"Palivo : pelety"]
[{"$nulls":5},"Dostupné farby: čierná , piesková, bordová"]
["Artel LS 8 IDRC - Keramika",{"$nulls":4},"cena : 2010,10 €"]
[{"$nulls":5},"Rozmery: (ŠxVxH) 605x1015x565 mm"]
[{"$nulls":5},"Hmotnosť : 100 kg"]
[{"$nulls":5},"Výkon : 10,1 kW"]
[{"$nulls":5},"Menovitý tepelný výkon : 3,88 - 8,54 kW"]
[{"$nulls":5},"Prívod vzduchu priemer rúry : 50 mm"]
[{"$nulls":5},"Priemer potrubia dymu zásuvky : 80 mm"]
[{"$nulls":5},"Vyhrievatelná plocha : 120 m2"]
[{"$nulls":5},"Doba samostatnej prevádzky : 6,5 - 14 hodín"]
[{"$nulls":5},"Palivo : pelety"]
[{"$nulls":5},"Dostupné farby: čierná , piesková, bordová"]
["Artel LS 6 M - Keramika",{"$nulls":4},"cena : 1337,15 €"]
[{"$nulls":5},"Rozmery: (ŠxVxH) 470x899x476 mm"]
[{"$nulls":5},"Hmotnosť   : 90 kg","90 kg"]
[{"$nulls":5},"Výkon : 8,4 kW"]
[{"$nulls":5},"Menovitý tepelný výkon : 4,97 - 7,12 kW"]
[{"$nulls":5},"Prívod vzduchu priemer rúry : 50 mm"]
[{"$nulls":5},"Priemer potrubia dymu zásuvky : 80 mm"]
[{"$nulls":5},"Vyhrievatelná plocha : 90 m2"]
[{"$nulls":5},"Doba samostatnej prevádzky : 8 - 13 hodín"]
[{"$nulls":5},"Palivo : pelety"]
[{"$nulls":5},"Dostupné farby: čierná , piesková, bordová"]
["Artel LS 8 M - Keramika",{"$nulls":4},"cena : 1540,17 €"]
[{"$nulls":5},"Rozmery: (ŠxVxH) 470x996x476 mm"]
[{"$nulls":5},"Hmotnosť :  100kg"]
[{"$nulls":5},"Výkon : 10,1 kW"]
[{"$nulls":5},"Menovitý tepelný výkon : 3,88 - 8,54 kW"]
[{"$nulls":5},"Prívod vzduchu priemer rúry : 50 mm"]
[{"$nulls":5},"Priemer potrubia dymu zásuvky : 80 mm"]
[{"$nulls":5},"Vyhrievatelná plocha : 120 m2"]
[{"$nulls":5},"Doba samostatnej prevádzky : 6,5 - 14 hodín"]
[{"$nulls":5},"Palivo : pelety"]
[{"$nulls":5},"Dostupné farby: čierná , piesková, bordová"]
["Artel LS 12 M - Keramika",{"$nulls":4},"cena : 2172,80 €"]
[{"$nulls":5},"Rozmery: (ŠxVxH) 534x1085x582 mm"]
[{"$nulls":5},"Hmotnosť :  160kg"]
[{"$nulls":5},"Výkon : 14,3 kW"]
[{"$nulls":5},"Menovitý tepelný výkon : 4,1 - 11,8 kW"]
[{"$nulls":5},"Prívod vzduchu priemer rúry : 50 mm"]
[{"$nulls":5},"Priemer potrubia dymu zásuvky : 80 mm"]
[{"$nulls":5},"Vyhrievatelná plocha : 140 m2"]
[{"$nulls":5},"Doba samostatnej prevádzky : 8,5 - 25 hodín"]
[{"$nulls":5},"Palivo : pelety"]
[{"$nulls":5},"Dostupné farby: čierná , piesková, bordová"]
[]
[]
[]
[]
["Artel LS 6 C - Keramika",{"$nulls":4},"cena : 1243,70 €"]
[{"$nulls":5},"Rozmery: (ŠxVxH) 470x899x476 mm"]
[{"$nulls":5},"Hmotnosť :  90kg"]
[{"$nulls":5},"Výkon : 8,4 kW"]
[{"$nulls":5},"Menovitý tepelný výkon : 4,97 - 7,12 kW"]
[{"$nulls":5},"Prívod vzduchu priemer rúry : 50 mm"]
[{"$nulls":5},"Priemer potrubia dymu zásuvky : 80 mm"]
[{"$nulls":5},"Vyhrievatelná plocha : 90 m2"]
[{"$nulls":5},"Doba samostatnej prevádzky : 8 - 13  hodín"]
[{"$nulls":5},"Palivo : pelety"]
[{"$nulls":5},"Dostupné farby: čierná , piesková, bordová"]
["Artel LS 8 C - Keramika",{"$nulls":4},"cena : 1444,71 €"]
[{"$nulls":5},"Rozmery: (ŠxVxH) 470x899x476 mm"]
[{"$nulls":5},"Hmotnosť :  100kg"]
[{"$nulls":5},"Výkon : 10,1 kW"]
[{"$nulls":5},"Menovitý tepelný výkon : 3,88 - 8,54 kW"]
[{"$nulls":5},"Prívod vzduchu priemer rúry : 50 mm"]
[{"$nulls":5},"Priemer potrubia dymu zásuvky : 80 mm"]
[{"$nulls":5},"Vyhrievatelná plocha : 120 m2"]
[{"$nulls":5},"Doba samostatnej prevádzky : 6,5 - 14  hodín"]
[{"$nulls":5},"Palivo : pelety"]
[{"$nulls":5},"Dostupné farby: čierná , piesková, bordová"]
["Artel LS 12 C - Keramika",{"$nulls":4},"cena : 2015,46 €"]
[{"$nulls":5},"Rozmery: (ŠxVxH) 534x1085x582 mm"]
[{"$nulls":5},"Hmotnosť :  160kg"]
[{"$nulls":5},"Výkon : 14,3 kW"]
[{"$nulls":5},"Menovitý tepelný výkon : 4,1 - 11,8 kW"]
[{"$nulls":5},"Prívod vzduchu priemer rúry : 50 mm"]
[{"$nulls":5},"Priemer potrubia dymu zásuvky : 80 mm"]
[{"$nulls":5},"Vyhrievatelná plocha : 140 m2"]
[{"$nulls":5},"Doba samostatnej prevádzky : 8,5 - 25  hodín"]
[{"$nulls":5},"Palivo : pelety"]
[{"$nulls":5},"Dostupné farby: čierná , piesková, bordová"]
["Artel LS 6 A - Oceľ",{"$nulls":4},"cena : 1149,60 €"]
[{"$nulls":5},"Rozmery: (ŠxVxH) 470x899x476 mm"]
[{"$nulls":5},"Hmotnosť :  90 kg"]
[{"$nulls":5},"Výkon : 8,4 kW"]
[{"$nulls":5},"Menovitý tepelný výkon : 4,97 - 7,12 kW"]
[{"$nulls":5},"Prívod vzduchu priemer rúry : 50 mm"]
[{"$nulls":5},"Priemer potrubia dymu zásuvky : 80 mm"]
[{"$nulls":5},"Vyhrievatelná plocha : 90 m2"]
[{"$nulls":5},"Doba samostatnej prevádzky : 8 - 13  hodín"]
[{"$nulls":5},"Palivo : pelety"]
[{"$nulls":5},"Dostupné farby: čierná , piesková, bordová"]
["Artel LS 8 A - Oceľ",{"$nulls":4},"cena : 1263,90 €"]
[{"$nulls":5},"Rozmery: (ŠxVxH) 470x899x476 mm"]
[{"$nulls":5},"Hmotnosť :  100 kg"]
[{"$nulls":5},"Výkon : 10,1 kW"]
[{"$nulls":5},"Menovitý tepelný výkon : 3,88 - 8,54 kW"]
[{"$nulls":5},"Prívod vzduchu priemer rúry : 50 mm"]
[{"$nulls":5},"Priemer potrubia dymu zásuvky : 80 mm"]
[{"$nulls":5},"Vyhrievatelná plocha : 120 m2"]
[{"$nulls":5},"Doba samostatnej prevádzky : 6,5 - 14  hodín"]
[{"$nulls":5},"Palivo : pelety"]
[{"$nulls":5},"Dostupné farby: čierná , piesková, bordová"]
[]
[]
[]
[]
[]
["Artel LS 12 A - Oceľ",{"$nulls":4},"cena : 1808,40 €"]
[{"$nulls":5},"Rozmery: (ŠxVxH) 534x1085x582 mm"]
[{"$nulls":5},"Hmotnosť :  160 kg"]
[{"$nulls":5},"Výkon : 14,3 kW"]
[{"$nulls":5},"Menovitý tepelný výkon : 4,1 - 11,8 kW"]
[{"$nulls":5},"Prívod vzduchu priemer rúry : 50 mm"]
[{"$nulls":5},"Priemer potrubia dymu zásuvky : 80 mm"]
[{"$nulls":5},"Vyhrievatelná plocha : 140 m2"]
[{"$nulls":5},"Doba samostatnej prevádzky : 8,5 - 25  hodín"]
[{"$nulls":5},"Palivo : pelety"]
[{"$nulls":5},"Dostupné farby: čierná , piesková, bordová"]
["Artel LSC 12 M - Top keramika",{"$nulls":4},"cena : 2393,30 €"]
[{"$nulls":5},"Rozmery: (ŠxVxH) 534x1085x582 mm"]
[{"$nulls":5},"Hmotnosť :  160 kg"]
[{"$nulls":5},"Výkon : 14,3 kW"]
[{"$nulls":5},"Menovitý tepelný výkon : 4,1 - 11,8 kW"]
[{"$nulls":5},"Prívod vzduchu priemer rúry : 50 mm"]
[{"$nulls":5},"Priemer potrubia dymu zásuvky : 80 mm"]
[{"$nulls":5},"Vyhrievatelná plocha : 140 m2"]
[{"$nulls":5},"Doba samostatnej prevádzky : 8,5 - 25  hodín"]
[{"$nulls":5},"Palivo : pelety"]
[{"$nulls":5},"Dostupné farby: čierná , piesková, bordová"]
["Artel LSC 12 C - Keramika",{"$nulls":4},"cena : 2265,55 €"]
[{"$nulls":5},"Rozmery: (ŠxVxH) 534x1085x582 mm"]
[{"$nulls":5},"Hmotnosť :  160 kg"]
[{"$nulls":5},"Výkon : 14,3 kW"]
[{"$nulls":5},"Menovitý tepelný výkon : 4,1 - 11,8 kW"]
[{"$nulls":5},"Prívod vzduchu priemer rúry : 50 mm"]
[{"$nulls":5},"Priemer potrubia dymu zásuvky : 80 mm"]
[{"$nulls":5},"Vyhrievatelná plocha : 140 m2"]
[{"$nulls":5},"Doba samostatnej prevádzky : 8,5 - 25  hodín"]
[{"$nulls":5},"Palivo : pelety"]
[{"$nulls":5},"Dostupné farby: čierná , piesková, bordová"]
["Artel LSC 12 C - Oceľ",{"$nulls":4},"cena : 2084 €"]
[{"$nulls":5},"Rozmery: (ŠxVxH) 534x1085x582 mm"]
[{"$nulls":5},"Hmotnosť :  160 kg"]
[{"$nulls":5},"Výkon : 14,3 kW"]
[{"$nulls":5},"Menovitý tepelný výkon : 4,1 - 11,8 kW"]
[{"$nulls":5},"Prívod vzduchu priemer rúry : 50 mm"]
[{"$nulls":5},"Priemer potrubia dymu zásuvky : 80 mm"]
[{"$nulls":5},"Vyhrievatelná plocha : 140 m2"]
[{"$nulls":5},"Doba samostatnej prevádzky : 8,5 - 25  hodín"]
[{"$nulls":5},"Palivo : pelety"]
[{"$nulls":5},"Dostupné farby: čierná , piesková, bordová"]
{"$rows_empty":9}
["Teplovodné pece na pelety ARTEL"]
["Veľkoobchodný cenník bez DPH"]
[{"$nulls":4},"tel.: 0905 394055 , 046 5431611 , fax.: 046 5431612"]
[{"$nulls":4},"e-mail.: tumainvest@gmail.com"]
[{"$nulls":4},"web.: www.krby-tuma.sk"]
["Výhradný distribútor ARTEL pre SR "]
["Artel LST 20/12 M - Top keramika",{"$nulls":4},"cena : "]
[{"$nulls":5},"Rozmery: (ŠxVxH) 534x1085x582 mm"]
[{"$nulls":5},"Hmotnosť :  160 kg"]
[{"$nulls":5},"Výkon : 14,1 kW"]
[{"$nulls":5},"Menovitý teplovodný výkon : 5,5 - 12,8 kW"]
[{"$nulls":5},"Prívod vzduchu priemer rúry : 50 mm"]
[{"$nulls":5},"Priemer potrubia dymu zásuvky : 80 mm"]
[{"$nulls":5},"Vyhrievatelná plocha : 140 m2"]
[{"$nulls":5},"Doba samostatnej prevádzky : 5 - 25  hodín"]
[{"$nulls":5},"Účinnosť:  94 %"]
[{"$nulls":5},"Palivo : pelety"]
[{"$nulls":5},"Dostupné farby: čierná , piesková, bordová"]
["Artel LST 20/12 C - Keramika",{"$nulls":4},"cena : "]
[{"$nulls":5},"Rozmery: (ŠxVxH) 534x1085x582 mm"]
[{"$nulls":5},"Hmotnosť :  160 kg"]
[{"$nulls":5},"Výkon : 14,1 kW"]
[{"$nulls":5},"Menovitý teplovodný výkon : 5,5 - 12,8 kW"]
[{"$nulls":5},"Prívod vzduchu priemer rúry : 50 mm"]
[{"$nulls":5},"Priemer potrubia dymu zásuvky : 80 mm"]
[{"$nulls":5},"Vyhrievatelná plocha : 140 m2"]
[{"$nulls":5},"Doba samostatnej prevádzky : 5 - 25  hodín"]
[{"$nulls":5},"Účinnosť:  94 %"]
[{"$nulls":5},"Palivo : pelety"]
[{"$nulls":5},"Dostupné farby: čierná , piesková, bordová"]
["Artel LST 20/12 C - Oceľ",{"$nulls":4},"cena : "]
[{"$nulls":5},"Rozmery: (ŠxVxH) 534x1085x582 mm"]
[{"$nulls":5},"Hmotnosť :  160 kg"]
[{"$nulls":5},"Výkon : 14,1 kW"]
[{"$nulls":5},"Menovitý teplovodný výkon : 5,5 - 12,8 kW"]
[{"$nulls":5},"Prívod vzduchu priemer rúry : 50 mm"]
[{"$nulls":5},"Priemer potrubia dymu zásuvky : 80 mm"]
[{"$nulls":5},"Vyhrievatelná plocha : 140 m2"]
[{"$nulls":5},"Doba samostatnej prevádzky : 5 - 25  hodín"]
[{"$nulls":5},"Účinnosť:  94 %"]
[{"$nulls":5},"Palivo : pelety"]
[{"$nulls":5},"Dostupné farby: čierná , piesková, bordová"]
["Artel LST 20/16 M - Top keramika",{"$nulls":4},"cena : 2951,30 € "]
[{"$nulls":5},"Rozmery: (ŠxVxH) 534x1085x582 mm"]
[{"$nulls":5},"Hmotnosť :  180 kg"]
[{"$nulls":5},"Výkon : 17,9 kW"]
[{"$nulls":5},"Menovitý teplovodný výkon : 6,5 - 16,3 kW"]
[{"$nulls":5},"Prívod vzduchu priemer rúry : 50 mm"]
[{"$nulls":5},"Priemer potrubia dymu zásuvky : 80 mm"]
[{"$nulls":5},"Vyhrievatelná plocha : 150 m2"]
[{"$nulls":5},"Doba samostatnej prevádzky : 7 - 17  hodín"]
[{"$nulls":5},"Účinnosť:  94 %"]
[{"$nulls":5},"Palivo : pelety"]
[{"$nulls":5},"Dostupné farby: čierná , piesková, bordová"]
{"$rows_empty":10}
["Artel LST 20/16 C - Keramika",{"$nulls":4},"cena : 2816,80 € "]
[{"$nulls":5},"Rozmery: (ŠxVxH) 534x1085x582 mm"]
[{"$nulls":5},"Hmotnosť :  180 kg"]
[{"$nulls":5},"Výkon : 17,9 kW"]
[{"$nulls":5},"Menovitý teplovodný výkon : 6,5 - 16,3 kW"]
[{"$nulls":5},"Prívod vzduchu priemer rúry : 50 mm"]
[{"$nulls":5},"Priemer potrubia dymu zásuvky : 80 mm"]
[{"$nulls":5},"Vyhrievatelná plocha : 150 m2"]
[{"$nulls":5},"Doba samostatnej prevádzky : 7 - 17  hodín"]
[{"$nulls":5},"Účinnosť:  94 %"]
[{"$nulls":5},"Palivo : pelety"]
[{"$nulls":5},"Dostupné farby: čierná , piesková, bordová"]
["Artel LST 20/16 A - Oceľ",{"$nulls":4},"cena : 2615,10 € "]
[{"$nulls":5},"Rozmery: (ŠxVxH) 534x1085x582 mm"]
[{"$nulls":5},"Hmotnosť :  180 kg"]
[{"$nulls":5},"Výkon : 17,9 kW"]
[{"$nulls":5},"Menovitý teplovodný výkon : 6,5 - 16,3 kW"]
[{"$nulls":5},"Prívod vzduchu priemer rúry : 50 mm"]
[{"$nulls":5},"Priemer potrubia dymu zásuvky : 80 mm"]
[{"$nulls":5},"Vyhrievatelná plocha : 150 m2"]
[{"$nulls":5},"Doba samostatnej prevádzky : 7 - 17  hodín"]
[{"$nulls":5},"Účinnosť:  94 %"]
[{"$nulls":5},"Palivo : pelety"]
[{"$nulls":5},"Dostupné farby: čierná , piesková, bordová"]
["Artel LST 20/20 M - Top keramika",{"$nulls":4},"cena : 3200,67 € "]
[{"$nulls":5},"Rozmery: (ŠxVxH) 534x1085x582 mm"]
[{"$nulls":5},"Hmotnosť :  185 kg"]
[{"$nulls":5},"Výkon : 21,7 kW"]
[{"$nulls":5},"Menovitý teplovodný výkon : 7,7 - 19,4 kW"]
[{"$nulls":5},"Prívod vzduchu priemer rúry : 50 mm"]
[{"$nulls":5},"Priemer potrubia dymu zásuvky : 80 mm"]
[{"$nulls":5},"Vyhrievatelná plocha : 180 m2"]
[{"$nulls":5},"Doba samostatnej prevádzky : 5,5 - 15  hodín"]
[{"$nulls":5},"Účinnosť:  94 %"]
[{"$nulls":5},"Palivo : pelety"]
[{"$nulls":5},"Dostupné farby: čierná , piesková, bordová"]
["Artel LST 20/20 C - Keramika",{"$nulls":4},"cena : 3052,80 € "]
[{"$nulls":5},"Rozmery: (ŠxVxH) 534x1085x582 mm"]
[{"$nulls":5},"Hmotnosť :  185 kg"]
[{"$nulls":5},"Výkon : 21,7 kW"]
[{"$nulls":5},"Menovitý teplovodný výkon : 7,7 - 19,4 kW"]
[{"$nulls":5},"Prívod vzduchu priemer rúry : 50 mm"]
[{"$nulls":5},"Priemer potrubia dymu zásuvky : 80 mm"]
[{"$nulls":5},"Vyhrievatelná plocha : 180 m2"]
[{"$nulls":5},"Doba samostatnej prevádzky : 5,5 - 15  hodín"]
[{"$nulls":5},"Účinnosť:  94 %"]
[{"$nulls":5},"Palivo : pelety"]
[{"$nulls":5},"Dostupné farby: čierná , piesková, bordová"]
["Artel LST 20/20 A - Oceľ",{"$nulls":4},"cena : 2837,65 € "]
[{"$nulls":5},"Rozmery: (ŠxVxH) 534x1085x582 mm"]
[{"$nulls":5},"Hmotnosť :  185 kg"]
[{"$nulls":5},"Výkon : 21,7 kW"]
[{"$nulls":5},"Menovitý teplovodný výkon : 7,7 - 19,4 kW"]
[{"$nulls":5},"Prívod vzduchu priemer rúry : 50 mm"]
[{"$nulls":5},"Priemer potrubia dymu zásuvky : 80 mm"]
[{"$nulls":5},"Vyhrievatelná plocha : 180 m2"]
[{"$nulls":5},"Doba samostatnej prevádzky : 5,5 - 15  hodín"]
[{"$nulls":5},"Účinnosť:  94 %"]
[{"$nulls":5},"Palivo : pelety"]
[{"$nulls":5},"Dostupné farby: čierná , piesková, bordová"]

{"sheet":"Hárok2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"Hárok3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}